{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","工作表"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"工作表","index":2,"n_rows":4,"n_cols":5,"rows_kept":4,"merged":[[0,0,0,4],[3,0,3,4]],"flags":["formulas_cached_only"]}
["中华人民共和国揭阳海关委托第三方编制“汕头海关老旧设施维修改造项目--揭阳海关”初步设计及投资概算、施工图项目报价清单"]
["序号","项目内容","服务期","下调比例","备注"]
[1,"对“汕头海关老旧设施维修改造项目—揭阳海关”项目提供包括但不限于编制项目初步设计和投资概算（上级部门批复前）、施工图（上级部门批复后）等服务。","自合同生效之日起至项目竣工验收合格之日止",null,"由供应商自报下浮率的形式报价并作为结算依据，该项目的结算执行计价格〔2002〕10号文，设计费计费基数为项目预算建安费，复杂系数、专业系数、附加调整系数等所有系数按1.0。设计费计费基数以我关委托的造价咨询机构审核为准。"]
["项目初步设计及投资概算、施工图包括但不限于以下内容：\n（一）综合业务用房/消除安全隐患\n1.各栋天面补漏、外墙翻新补漏、室内补漏、天花墙面刮涂。包括天面修缮，铲除防水隔热层，重新找坡，清洗批砂浆，新做防水隔热层，批砂浆保护，铺贴隔热砖；外墙翻新补漏，铲除外墙原有面层，局部防水处理，外墙面油漆；室内天花墙面油漆，局部渗漏修补。\n2.更换办公楼电梯。1台。\n3.油浸式变压器改造为干式变压器。1项。\n4.消火栓系统改造修缮-主楼、武警楼、新阳路办公区，更换老旧消火栓及配套设施及镀锌钢管消防管，新增消火栓连锁启泵系统。\n（二）生活保障设施/恢复使用功能\n1.海关宿舍小区现有6套公有住房修缮，恢复居住功能。\n（三）海关大门翻新，含外轮廓亮化（单面），铸铝定制徽标，更换老旧外饰面及龙骨，大门外墙清洗，内墙重新刷白等。"]